Huỳnh Ngọc Quang – SE181838

NWC204 - dunglt92

Lab - Use Wireshark to View Network Traffic

# Instructions

## Capture and Analyze Local ICMP Data in Wireshark

In Part 1 of this lab, you will ping another PC on the LAN and capture ICMP requests and replies in Wireshark. You will also look inside the frames captured for specific information. This analysis should help to clarify how packet headers are used to transport data to their destination.

### Retrieve your PC interface addresses.

For this lab, you will need to retrieve your PC IP address and its network interface card (NIC) physical address, also called the MAC address.

Open a Windows command prompt.

* + - 1. In a command prompt window, enter **ipconfig /all**, to the IP address of your PC interface, its description, and its MAC (physical) address.

A screenshot of a computer

Description automatically generated

* + - 1. Ask a team member or team members for their PC IP address and provide your PC IP address to them. Do not provide them with your MAC address at this time.

Close a Windows Command Prompt.

### Start Wireshark and begin capturing data.

* + - 1. Navigate to Wireshark. Double-click the desired interface to start the packet capture. Make sure the desired interface has traffic.
      2. Information will start scrolling down the top section in Wireshark. The data lines will appear in different colors based on protocol.

This information can scroll by very quickly depending on what communication is taking place between your PC and the LAN. We can apply a filter to make it easier to view and work with the data that is being captured by Wireshark.

For this lab, we are only interested in displaying ICMP (ping) PDUs. Type **icmp** in the **Filter** box at the top of Wireshark and press **Enter,** or click the **Apply** button (arrow sign) to view only ICMP (ping) PDUs.

* + - 1. This filter causes all data in the top window to disappear, but you are still capturing the traffic on the interface. Navigate to a command prompt window and ping the IP address that you received from your team member.

A computer screen shot of a computer screen

Description automatically generatedNotice that you start seeing data appear in the top window of Wireshark again.

A screenshot of a computer

Description automatically generated

**Note**: If the PC of your team member does not reply to your pings, this may be because the PC firewall of the team member is blocking these requests. Please see Appendix A: Allowing ICMP Traffic Through a Firewall for information on how to allow ICMP traffic through the firewall using Windows.

* + - 1. Stop capturing data by clicking the **Stop Capture** icon.

### Examine the captured data.

In Step 3, examine the data that was generated by the ping requests of your team member PC. Wireshark data is displayed in three sections: 1) The top section displays the list of PDU frames captured with a summary of the IP packet information listed; 2) the middle section lists PDU information for the frame selected in the top part of the screen and separates a captured PDU frame by its protocol layers; and 3) the bottom section displays the raw data of each layer. The raw data is displayed in both hexadecimal and decimal form.

* + - 1. Click the first ICMP request PDU frames in the top section of Wireshark. Notice that the **Source** column has your PC IP address, and the **Destination** column contains the IP address of the teammate PC that you pinged.
      2. With this PDU frame still selected in the top section, navigate to the middle section. Click the plus sign to the left of the Ethernet II row to view the destination and source MAC addresses.

#### Questions:

Does the source MAC address match your PC interface?

Yes

Does the destination MAC address in Wireshark match your team member MAC address?

Yeshere.

How is the MAC address of the pinged PC obtained by your PC?

The MAC address is obtained through an ARP request.

**Note**: In the preceding example of a captured ICMP request, ICMP data is encapsulated inside an IPv4 packet PDU (IPv4 header) which is then encapsulated in an Ethernet II frame PDU (Ethernet II header) for transmission on the LAN.

## Capture and Analyze Remote ICMP Data in Wireshark

In Part 2, you will ping remote hosts (hosts not on the LAN) and examine the generated data from those pings. You will then determine what is different about this data from the data examined in Part 1.

### Start capturing data on the interface.

* + - 1. Start the data capture again.
      2. A window prompts you to save the previously captured data before starting another capture. It is not necessary to save this data. Click **Continue without Saving**.
      3. With the capture active, ping the following three website URLs from a Windows command prompt:

Open a Windows command prompt

* + - * 1. www.yahoo.com
        2. www.cisco.com
        3. www.google.com

**Note**: When you ping the URLs listed, notice that the Domain Name Server (DNS) translates the URL to an IP address. Note the IP address received for each URL.

* + - 1. You can stop capturing data by clicking the **Stop Capture** icon.

A screenshot of a computer screen

Description automatically generated

### Examining and analyzing the data from the remote hosts.

Review the captured data in Wireshark and examine the IP and MAC addresses of the three locations that you pinged. List the destination IP and MAC addresses for all three locations in the space provided.

#### Questions:

IP address for **www.yahoo.com**:

202.165.107.49

MAC address for **www.yahoo.com**:

***58:9b:4a:2e:c4:54***

IP address for **www.cisco.com**:

23.77.60.96

MAC address for **www.cisco.com**:

58:9b:4a:2e:c4:54

IP address for **www.google.com**:

142.250.66.100

MAC address for **www.google.com**:

***58:9b:4a:2e:c4:54***

What is significant about this information?

***The MAC addresses for all three locations are the same (Router MAC).***

How does this information differ from the local ping information you received in Part 1?

1. **A local host ping provides the MAC address of the PC's network interface card (NIC), while a ping to a remote host yields the MAC address of the LAN interface on the default gateway.**

# Reflection Question

Why does Wireshark show the actual MAC address of the local hosts, but not the actual MAC address for the remote hosts?

When dealing with remote hosts on the local network, their MAC addresses are typically unknown. In such cases, the MAC address of the default gateway is employed. Once the packet arrives at the default gateway router, the Layer 2 information is removed from the packet, and a fresh Layer 2 header is affixed, containing the destination MAC address of the next-hop router.

# Appendix A: Allowing ICMP Traffic Through a Firewall

If the members of your team are unable to ping your PC, the firewall may be blocking those requests. This appendix describes how to create a rule in the firewall to allow ping requests. It also describes how to disable the new ICMP rule after you have completed the lab.

## Create a new inbound rule allowing ICMP traffic through the firewall.

* + - 1. Navigate to the **Control Panel** and click the **System and Security** option in the Category view.
      2. In the **System and Security** window, click **Windows Defender Firewall** or **Windows Firewall**.
      3. In the left pane of the **Windows Defender Firewall** or **Windows Firewall** window, click **Advanced settings**.
      4. On the **Advanced Security** window, click the **Inbound Rules** option on the left sidebar and then click **New Rule…** on the right sidebar.
      5. This launches the **New Inbound Rule** wizard. On the **Rule Type** screen, click the **Custom** radio button and click **Next**.
      6. In the left pane, click the **Protocol and Ports** option and using the **Protocol Type** drop-down menu, select **ICMPv4**, and then click **Next**.
      7. Verify that **Any IP address** for both the local and remote IP addresses are selected. Click **Next** to continue.
      8. Select **Allow the connection**. Click **Next** to continue.
      9. By default, this rule applies to all the profiles. Click **Next** to continue.
      10. Name the rule with **Allow ICMP Requests**. Click **Finish** to continue. This new rule should allow your team members to receive ping replies from your PC.

## Disabling or deleting the new ICMP rule.

After the lab is complete, you may want to disable or even delete the new rule you created in Step 1. Using the **Disable Rule** option allows you to enable the rule again at a later date. Deleting the rule permanently deletes it from the list of inbound rules.

* + - 1. On the **Advanced Security** window, click **Inbound Rules** in the left pane and then locate the rule you created previously.
      2. Right-click the ICMP rule and select **Disable Rule** if so desired. You may also select **Delete** if you want to permanently delete it. If you choose this option, you must re-create the rule again to allow ICMP replies.End of document